/*
 * FreeRTOS Kernel V10.2.1
 * Copyright (C) 2019 Amazon.com, Inc. or its affiliates.  All Rights Reserved.
 *
 * Permission is hereby granted, free of charge, to any person obtaining a copy of
 * this software and associated documentation files (the "Software"), to deal in
 * the Software without restriction, including without limitation the rights to
 * use, copy, modify, merge, publish, distribute, sublicense, and/or sell copies of
 * the Software, and to permit persons to whom the Software is furnished to do so,
 * subject to the following conditions:
 *
 * The above copyright notice and this permission notice shall be included in all
 * copies or substantial portions of the Software.
 *
 * THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR
 * IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY, FITNESS
 * FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR
 * COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER
 * IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN
 * CONNECTION WITH THE SOFTWARE OR THE USE OR OTHER DEALINGS IN THE SOFTWARE.
 *
 * http://www.FreeRTOS.org
 * http://aws.amazon.com/freertos
 *
 * 1 tab == 4 spaces!
 */
#include "FreeRTOSConfig.h"
#include "portasm.h"

	IMPORT xTaskIncrementTick
	IMPORT vTaskSwitchContext
	IMPORT vPortSetupTimerInterrupt

	EXPORT vTickISR
	EXPORT vPortYield
	EXPORT xPortStartScheduler

	RSEG CODE

/*
 * The RTOS tick ISR.
 *
 * If the cooperative scheduler is in use this simply increments the tick
 * count.
 *
 * If the preemptive scheduler is in use a context switch can also occur.
 */
vTickISR:
	portSAVE_CONTEXT

	call	#xTaskIncrementTick
	cmp.w	#0x0, R12
    jeq		SkipContextSwitch
	call	#vTaskSwitchContext
SkipContextSwitch:

	portRESTORE_CONTEXT
/*-----------------------------------------------------------*/


/*
 * Manual context switch called by the portYIELD() macro.
 */
vPortYield:

	/* Mimic an interrupt by pushing the SR. */
	push	SR

	/* Now the SR is stacked we can disable interrupts. */
	dint

	/* Save the context of the current task. */
	portSAVE_CONTEXT

	/* Switch to the highest priority task that is ready to run. */
	call	#vTaskSwitchContext

	/* Restore the context of the new task. */
	portRESTORE_CONTEXT
/*-----------------------------------------------------------*/


/*
 * Start off the scheduler by initialising the RTOS tick timer, then restoring
 * the context of the first task.
 */
xPortStartScheduler:

	/* Setup the hardware to generate the tick.  Interrupts are disabled
	when this function is called. */
	call	#vPortSetupTimerInterrupt

	/* Restore the context of the first task that is going to run. */
	portRESTORE_CONTEXT
/*-----------------------------------------------------------*/


	/* Install vTickISR as the timer A0 interrupt. */
	ASEG
	ORG 0xFFE0 + TIMERA0_VECTOR

	_vTickISR_: DC16 vTickISR


	END

