`include "gpio.rdl"
`include "uart.rdl"
`include "spi.rdl"
`include "pwm.rdl"
`include "plic.rdl"
`include "aon.rdl"
`include "prci.rdl"
`include "clint.rdl"

addrmap e300_plat_t {
	lsb0;
	clint_regs clint @0x02000000;
    plic_regs  plic  @0x0C000000;
    aon_regs   aon   @0x10000000;
    prci_regs  prci  @0x10008000;
    gpio_regs  gpio0 @0x10012000;
    uart_regs  uart0 @0x10013000;
    spi_regs   qspi0 @0x10014000;  
    pwm_regs   pwm0  @0x10015000;
    uart_regs  uart1 @0x10023000;
    spi_regs   qspi1 @0x10024000;  
    pwm_regs   pwm1  @0x10025000;
    spi_regs   qspi2 @0x10034000;  
    pwm_regs   pwm2  @0x10035000;
} e300_plat;
